	Video & High Power UTP Cabling Solution 


ITEM NO.:  TTA111VPDK (TTP111VPDC + TTA111VPDR)  
TTA111VPDK Kit is special design to use standard CAT5 & RJ45 structured building wiring to carry video, High DC power and data for simplifying short range installation by centralizing power and reducing installation labor costs, including TTP111VPDC transmitter and TTA111VPDR receiver in one package.  TTA111VPDR receiver built in high DC power supply working with TTP111VPDC as transmitter at camera side could support camera loads up to 1.5Amp per channel at distance 300 meters.  With data transmission which is perfect for PTZ camera application.  
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TTP111VPDC   Video, Power, Data Transmitter Built in DC12V Power regulator  
· To send video and remote power over one UTP CAT5 cable.

· Built in RS485 terminal for data transmission. 

· Built in power detection with power output DC12V regulated 1.5Amp at 300 meters.
· Built in fan for low operating temperature.
· Transmission distance up to 300 meters.

· Built in LED indication.

· Built in ESD and surge protection.

· For DC12V camera use, the power sources from remote UTP receiver: TTA111VPDR, TTA414VPDR for professional CCTV Industry Installation.                     
TTA111VPDR   1 Port Video, Power, Data Receiver With DC High Power Supply 
· Use with TTP111VPDC video, power, data transmitter at camera side to send video and power, data from remote side over over one UTP CAT5 cable..

· RJ45 termination for easy installation.

· Provide high power to remote camera DC12V/25W (Max.) 

· Power input: AC100-AC240V. 

· Transmission range up to 300 meters.

· Built in LED indication.

· Built in ESD and surge protection.

Installation View:
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TTP111VPDC, TTA111VPDR, LED:
Blue (front panel): power on/off

TTA111VPDR,  RJ45 LED Indication:
Green :
 Power Output Normal
Yellow :   Video Detection
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Power Distance Chart：
The distance will be affected by cable quality. 
	50 M
	DC12V/2Amp

	100M
	DC12V/1.7Amp

	200M
	DC12V/1.6Amp

	300M
	1.5Amp


Product Overview:
TTP111VPDC
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TTA111VPDR
 [image: image7.jpg]Video,PowerData  RS485  VIDEOOUT

@Ml@

ACI100~240V





Caution:  to avoid any damage, TTP111VPDC, TTA111VPDR, cabling is not able to connect any Ethernet or PoE network with outside plant routing. 

Specification:
	ITEM NO.
	TTP111VPDC

	Video, Input
	BNC, 1Vp-p, 75ohm

	Data Input
	RS485 Terminal Block

	Video, Data, Power Transmission
	RJ45 Termination

	LED Indication
	Power: Blue color

	RJ45 Pin Define
	Video: pin 7.8, Data: pin 1, 2, Power: pin 3,4,5.6,

	Output Power
	12V, 1.5Amp ( Max)

	Power Consumption
	3W ( Max.)

	Distance
	300 M

	Recommend Cable
	CAT 5 Cable 4 Pairs (24 AWG)

	Temperature 
	Operation: 0 to 55℃, Storage: -20 TO 85℃, Humidity: up to 95%

	Dimension     W x H x D mm
	113.5 x 117 x 36

	Weight                  g
	400 g


	ITEM NO.
	TTA11VPDR

	Video, Input
	BNC, 1Vp-p, 75ohm

	Data Input
	RS485 Terminal Block

	Video, Data, Power Transmission
	RJ45 Termination

	LED Indication
	Power: blue , Power output: green, Video: yellow

	RJ45 Pin Define
	Video: pin 7.8, Data: pin 1, 2, Power: pin 3,4,5.6,

	Power  
	Input: AC110-AC240V, Output: 54V

	Power Consumption
	2W ( Max.)

	Distance
	300 M

	Recommend Cable
	CAT 5 Cable 4 Pairs (24 AWG)

	Temperature 
	Operation: 0 to 55℃, Storage: -20 TO 85℃, Humidity: up to 95%

	Dimension     W x H x D mm
	117.7 x 117 x 36

	Weight                  g
	450 g
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